# Audio System Programming Options

General Options
Unit Operation: | Event Priority:
FACP Data Bus Control: | FACP Data Bus Address (0-32):
24 Hour Resound: | Canadian Configuration:
Class A / Style Z: | Canadian Isolator Modules:
AC Loss Delay (Hours): | Secondary Amplifier:
Primary Amp 25/70 VAC: | Secondary Amp 25/70 VAC:
External Audio Input: | IP Address:
Identification:

NAC Options
NAC Type: | NAC Protocol:
Aux Power: | Speaker Volume Control NAC:
Active With Page: | Page Timeout (Seconds):

Console Control
Console Priority:
Device Control Timeout (30-300 Seconds):
Paging Timeout (30-300 Seconds):
UFC Event Timeout (0-240 Minutes):
RM/RPU for UFC Applications: